TOOLBOX TALK 15 • SUPERVISOR COMPONENT
Supervisor Field Check
Hearing Protection: Control Noise, Check the Fit | v1.0 | October 6, 2026
Task / location: __________________________________________________________
Date / time / shift: __________________  Leader: ______________________________
JHA/JSA reference / revision: _______________________________________________
Change or conditions confirmed unchanged: ___________________________________
Short leader check
Mark V = verified, H = hold/not verified, or N/A with a reason. Support each result with evidence below or a referenced task record; a blank is not a pass.
	Check
	V / H / N/A

	Current noise assessment covers task, duration, enclosure and adjacent work.
	

	Specified engineering/work controls are present and usable.
	

	Selected protectors and attenuation evaluation match the exposure.
	

	Individual fitting checked with other PPE; defects or interference resolved.
	

	Communication, symptom reporting and reassessment triggers understood.
	



Control verification — attach more rows for all required controls
	Control / exposure
	Source, revision & criterion
	Safe method / verifier
	Actual result / time / status

	
	
	
	

	
	
	
	

	
	
	
	



Use applicable regulatory, manufacturer, procedure, permit or engineering criteria. Only appropriately competent and authorized people perform checks; do not improvise tests or enter danger to verify protection.
Unresolved item / restriction: _________________________________________________
Action owner / due before exposure: __________________________________________
Correction / recheck result and time: __________________________________________
Stop contact: ____________________  Restart authority: ________________________
Next recheck trigger: ____________________  Crew rebrief completed: ______________
Disposition: [ ] HOLD affected work  [ ] Checks complete; required approval confirmed
Approval / permit reference or justified N/A: ____________________________________
Leader / date / time: ______________________________________________________
Unverified required protection means HOLD. Correct, recheck, obtain required site authorization and rebrief before exposure.
This sheet supports the task plan. It does not replace required permits, inspections, specialist decisions or employer authorization.
Todd Jerome Jenkins  •  www.toddjeromejenkins.com  |  v1.0  |  




