TOOLBOX TALK 17 • SUPERVISOR COMPONENT
Supervisor Field Check
Wet Concrete: Prevent Skin and Eye Contact | v1.0 | October 6, 2026
Task / location: __________________________________________________________
Date / time / shift: __________________  Leader: ______________________________
JHA/JSA reference / revision: _______________________________________________
Change or conditions confirmed unchanged: ___________________________________
Short leader check
Mark V = verified, H = hold/not verified, or N/A with a reason. Support each result with evidence below or a referenced task record; a blank is not a pass.
	Check
	V / H / N/A

	Current product SDS and exposure assessment available.
	

	Work method limits skin contact and addresses necessary kneeling.
	

	PPE model suitability, fit, condition and clean interiors confirmed.
	

	Washing and required emergency flushing arrangements checked in place.
	

	Replacement items, contamination response and medical-help route ready.
	



Control verification — attach more rows for all required controls
	Control / exposure
	Source, revision & criterion
	Safe method / verifier
	Actual result / time / status

	
	
	
	

	
	
	
	

	
	
	
	



Use applicable regulatory, manufacturer, procedure, permit or engineering criteria. Only appropriately competent and authorized people perform checks; do not improvise tests or enter danger to verify protection.
Unresolved item / restriction: _________________________________________________
Action owner / due before exposure: __________________________________________
Correction / recheck result and time: __________________________________________
Stop contact: ____________________  Restart authority: ________________________
Next recheck trigger: ____________________  Crew rebrief completed: ______________
Disposition: [ ] HOLD affected work  [ ] Checks complete; required approval confirmed
Approval / permit reference or justified N/A: ____________________________________
Leader / date / time: ______________________________________________________
Unverified required protection means HOLD. Correct, recheck, obtain required site authorization and rebrief before exposure.
This sheet supports the task plan. It does not replace required permits, inspections, specialist decisions or employer authorization.
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