TOOLBOX TALK 18 • SUPERVISOR COMPONENT
Supervisor Field Check
Hand Protection: Match the Glove to the Task | v1.0 | October 6, 2026
Task / location: __________________________________________________________
Date / time / shift: __________________  Leader: ______________________________
JHA/JSA reference / revision: _______________________________________________
Change or conditions confirmed unchanged: ___________________________________
Short leader check
Mark V = verified, H = hold/not verified, or N/A with a reason. Support each result with evidence below or a referenced task record; a blank is not a pass.
	Check
	V / H / N/A

	Task and remaining hand hazards identified after stronger controls.
	

	Exact glove model matched to task and documented selection.
	

	Chemical conditions and replacement/use limits verified where relevant.
	

	Condition, fit, grip and compatibility with the method checked safely.
	

	Entanglement restrictions, replacement supply and stop response understood.
	



Control verification — attach more rows for all required controls
	Control / exposure
	Source, revision & criterion
	Safe method / verifier
	Actual result / time / status

	
	
	
	

	
	
	
	

	
	
	
	



Use applicable regulatory, manufacturer, procedure, permit or engineering criteria. Only appropriately competent and authorized people perform checks; do not improvise tests or enter danger to verify protection.
Unresolved item / restriction: _________________________________________________
Action owner / due before exposure: __________________________________________
Correction / recheck result and time: __________________________________________
Stop contact: ____________________  Restart authority: ________________________
Next recheck trigger: ____________________  Crew rebrief completed: ______________
Disposition: [ ] HOLD affected work  [ ] Checks complete; required approval confirmed
Approval / permit reference or justified N/A: ____________________________________
Leader / date / time: ______________________________________________________
Unverified required protection means HOLD. Correct, recheck, obtain required site authorization and rebrief before exposure.
This sheet supports the task plan. It does not replace required permits, inspections, specialist decisions or employer authorization.
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